İnductor turn ratio calculation

We need 1mH;

From the datasheet

Effective magnetic path length (l) =145mm

Effective cross-section area(A) = 158

Relative permeability = 2000